Wireless AG 3.1.3.5060 (Nov 25, 2004) Final

[Last version]
 * 3.1.3.5050

[Features Added]
 * Airpath compatibility.
 * iPass compatibility.

[Behavior Changes]
 
 * Default SSL certificate updated (Certificate Name: ag.interepoch.com.tw).
 * Web redirection related URLs expanded to 119 characters.
 * Web redirection related URLs such as Log-on and Log-off URL can be entered more friendly,
     ex:  1. www.x.com/index.htm
          2. http://www.x.com:8000/index.htm 
          3. https://www.x.com/index.htm

 * If the length of an ICMP ping echo request packet is more than 100 bytes,
   AG will block this ICMP packet to prevent unexpected attacks.
 * Stop sending ICMP responses for ICMP_DEST_UNREACHABLE to prevent unexpected attacks.
 * LAN Devices will be detected after system boot up 2 minutes, but can be managed immediately.

[Bugs Fixed]
    
 * LAN Device Management doesn't work when Web Redirection functionality has been enabled.
 * Bandwidth Control doesn't work properly.
 * 90015: After session timeout or idle timeout, the user can still connect to 
          the Internet without being authenticated again.
 * 90245: eBay links would make AG lock up.
 * 90252: Spelling error--"Periodioal Restart" in the Auto Recovery section.  
 * 90255: Some walled garden URLs (for example: www.microsoft.com) 
          can't be connected until the user is authenticated successfully.
 * 90256: DNS proxy can't work properly and it may cause AG to reboot or lock up.
 * 90257: Walled garden URLs are case-sensitive.
 * 90258: UPnP packets incoming from WAN ports are not blocked.
 
         
[Config version] 
 * CONFIG.DAT V23 30000

[Configuration File Convertor]
 * Yes, v5060 can be upgraded from v5004, v5013 and v5050.
 