Wireless AG 3.1.3.5050 (Sep 23, 2004) Final

[Last version]
* 3.1.3.5013

[Features Added]
* New wireless security mode: 802.1x PEAP 

[Behavior Changes]
* None.

[Bugs Fixed]
* 90130: Zero Client Reconfiguration does not work in some case. 
* 90131: LAN Device Management (from the AG) kept reporting that the DRAP was down. 
* 90147: DNS Client does not work properly sometimes. 
* 90154: VLAN tagged packets cause rebooting. 
* 90155: If WAN and LAN are connected to form a loop, buffer overflows occur and the device locks up.
* Unused ports are not blocked so that the device can be scanned by the following applications
  from the WAN side:
  - http://scan.sygate.com/prestealthscan.html
  - https://www.grc.com/x/ne.dll?bh0bkyd2
  - http://security.symantec.com
* Random rebooting in the following situations:
  - When the WAN interfaces are disconnected.
  - When DMZ is enabled.
  - When the administrator is using the Web UI for management purposes.
* The Web UI may not work.
* The AG may hang after firmware upgrade.
* Bugs regarding PPPoE operations.
* When DMZ is enabled, SNTP does not work.
* The device reboots when the administrator accesses the General, Password page of the Web UI.
* 90025: IPSec traffic cannot be passed through when using Netscreen VPN Client in Main mode.
* 90028: ifOutOctets of MIB II is always 0.
* 90061: IPSec traffic cannot be passed through when using Nortel Networks "Contivity VPN Client".
* 90147: DNS Client does not work properly sometimes.
* UDP packets with checksum value 0 would result in checksum errors. This bug may make
  voice applications (MSN, H.323, etc) not work properly sometime.
* 90195: The DHCP client of the device accepts only one DNS server even if the DHCP
  server of the ISP gives it 2 or more DNS servers.
* In the IP header of any multicast UDP message sent by the device, the TTL was set to 1,
  which makes some applications (ex. DHCP) not work sometime. The TTL value has been
  changed to 16.
* The "Cancel" button on the "LAN Device Management" page is inactive.
* In "Base64" password encryption method mode, the log-on page does not show smoothly.

[Configuration File Convertor]
* None.